____________________________________
	Skyboy Check List
____________________________________
Before Starting Engines

- Preflight Inspection: COMPLETE
- Seats, Seat Belts: ADJUST AND LOCK
- Lights: OFF
- Radios: OFF
- Fuel Shutoff Valve: ON
____________________________________
Starting Engine

- Parking Brake: SET
- Prime: AS REQUIRED (up to 3 strokes)
- Throttle: OPEN 1/2 INCH 
- Mixture: RICH
- Master Switch: ON
- Fuel Pump: ON
- Propeller Area: CLEAR
- Ignition Switch: START
- Throttle: ADJUST FOR 1000RPM OR LESS
- Oil Pressure: CHECK
- Oil Temperature: CHECK
- Navigation Lights: ON AS REQUIRED
- Flashing Beacon: ON AS REQUIRED
___________________________________
Before Take Off

- Seats, Seat Belts: CHECK SECURE
- Cabin Doors: CLOSED AND LATCHED
- Flight Controls: FREE AND CORRECT
- Flight Instruments: CHECK AND SET
- Fuel Quantity: CHECK
- Fuel Shutoff Valve: RECHECK ON
- Mixture: RICH (below 3000ft)
- Elevator Trim: SET FOR TAKEOFF
- Throttle: 1700RPM
- Magnetos: CHECK FOR RPM DROP
- Engine Instruments and Ammeter: CHECK
- Throttle: 1000RPM OR LESS
- Strobe Lights: AS DESIRED
- Radios and Avionics: SET
- Brakes: RELEASE
____________________________________
Takeoff

- Throttle: FULL OPEN
- Elevator Control: LIFT NOSE WHEEL AT 60 MPH
- Climb Speed: 65-75 MPH
- Mixture: RICH BELOW 3000FT, LEAN ABOVE 3000FT
____________________________________
Cruise

- Power: 1900-2550RPM (NO more than 75% recommended)
- Elevator Trim: ADJUST TO CENTER
- Mixture: LEAN (as required)
____________________________________
Before Landing

- Seats, Seat Belts: ADJUST AND LOCK
- Mixture: RICH
- Fuel Selector: BOTH
____________________________________
Landing

- Pattern speed: 85 MPH 
- Approach speed: 70 MPH
- Touchdown: MAIN WHEELS FIRST
- Landing Roll: LOWER NOSE WHEEL GENTLY
- Braking: MINIMUM REQUIRED
____________________________________
Securing Airplane

- Parking Brake: SET
- Lights: OFF
- Mixture: IDLE CUT-OFF
- Ignition Switch: OFF
- Fuel Pump: OFF
- Master Switch: OFF
